TABLE ROUTER

WARNING!

* Eye and ear protection required
* No loose clothing, tie back long hair
* Turn off the machine at the isolation switch when making any adjustments.
* Install bits with at least 15mm of the shaft in the collet chuck. Any less and the bit could vibrate loose during use.
* Make sure the bit is clear of the stock before turning on.
* Keep your hands and fingers at least 3” away from the bit.
* Take light cuts; larger cuts can result in kickback.
* ALWAYS cut against the rotation of the bit, feeding the material from the right to the left of the router table. This gives you better control and prevents the machine from pulling the stock into the bit.
* Use caution when cutting against the grain. Use the fence to decrease the depth of cut.