BANDSAW

WARNING!

* Eye and ear protection required
* No loose clothing, tie back long hair
* Turn off the machine at the isolation switch when making any adjustments.
* Lower guard so that the minimum amount of blade is exposed (1/2” above the work)
* Keep hands at least 4” away from the blade at all times. Ensure hands are to the side of the blade, not in line with the path of the cut. Use push sticks when needed.
* Plan your cuts carefully. Saw curves gradually. Make straight relief cuts prior to making curved cuts
* Do not back out of long cuts
* Do not operate the bandsaw from the side and do not stand to the side of the bandsaw while waiting to use the machine
* Do not leave the machine until the blade has stopped moving