TABLE SAW

WARNING!

* Eye and ear protection required
* No loose clothing or jewelry, tie back long hair
* For ripping, splitter must be used to prevent kickback, push sticks also must be used
* Guards must be in place at all times
* Keep hands clear a minimum of 6” of blade
* Never cut warped or bowed stock on this saw
* Limit the amount of exposed blade as much as possible
* When cutting long material, stock must be suspended at same level as saw table
* Push stock all the way through, clear of blade to prevent kickback
* Do not stand directly behind stock in case of kickback
* Securely lock in all angle settings
* Always use isolation switch or unplug machine when changing blade.